          Wiring ERIS A30 with U-Link 2.0 boards ( Tested – 5 wires)

- Insert the battery ONLY after all the wiring and settings have been done
- Make sure all the jumpers (the shunts) are left open, as they come from the factory
- Make sure the photocells are aligned by following the specific alignment paragraph on the full instruction
- Only remove the link between 70-72 on the control board and leave the others in place (70-71 & 70-73)
- On control boards with an LCD display, set in the Logic menu SAFE1 to 005 and press OK to confirm 
- On control boards without LCD display, flick the dip-switch 3 & 4 to UP position (IO config)
and press the button S2 for more than 5sec to confirm

[image: ]
Please note that the battery side TX goes into low power mode  in open position and in close position it shuts down PE beams   
This wiring is Ecosol compatible 
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