          Wiring ERIS A30 with U-Link 2.0 boards ( Untested – 4 wires)

- Insert the battery ONLY after all the wiring and settings have been done
- Keep power down activation active , [image: ]
- To maximize battery life on the PE(TX), it is recommended that the Auto Close function remains enabled.
- Make sure the photocells are aligned by following the specific alignment paragraph on the full instruction
- Only remove the link between 70-72 on the control board and leave the others in place (70-71 & 70-73)
- On control boards with an LCD display :
· Go to LOGIC menu and set 1 SAFE = 00 ( active in both opening and closing ) Press OK to confirm 
· Go to LOGIC menu and set 1 SAFE = 04 ( active in closing only ) press OK to confirm.
- On control boards without LCD display:
· For Photocell in active in opening and closing no change in dipswitch .
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