

[image: ] WIRING COMPACTA /AKTA PE BEAMS TO U-LINK 2.0 boards 

Activate PE beams in Closing only with tested wiring  : 
- Make sure the photocells are aligned
- Only remove the link between 70-72 on the control board and leave the others in place (70-71 & 70-73)
- On control boards without LCD display, flick the dip-switch 3 & 4  to UP position  (IO Config ) ) and press the button S2 for more than 5sec to confirm
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